                        SCI-100 COVE B

	SECTION 1. IDENTIFICATION

	Product identifier
	SCI-100 COVE B

	Other Means of Identification
	N. A

	Recommended Use
	Epoxy coating

	Restrictions on Use
	Unknown

	Supplier Identifier
	SCI COATINGS INC.
2821 Boulevard Le Corbusier Laval, Québec
Canada H7L 4J5
Web: www.scicoatings.com

	Emergency Phone No.
	24-Hour Emergency Telephone Number Canada (CANUTEC): (613) 996-6666



	SECTION 2. HAZARD IDENTIFICATION

	Classification
	Acute Toxicity, Oral Category 4 Skin Sensitization Category 1A
Skin Corrosion/irritation Category 1B Serious eye damage/irritation Category 1 Reproductive toxicity Category 2
Hazardous to the aquatic environment - acute Category 1 Hazardous to the aquatic environment - chronic Category 1

	Label Elements
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Signal Word
Danger

Hazard Statements
H302: Harmful if swallowed
H317: May cause an allergic skin reaction
H314: Causes severe skin burns and eye damage H318: Causes serious eye damage
H361: Suspected of damaging fertility or the unborn child H400: Very toxic to aquatic life
H410: Very toxic to aquatic life with long lasting effects
Precautionary statements
Prevention:
P201 Obtain special instructions before use. P202 Do not handle until all safety precautions have been read and understood. P260 Do not breathe dust or mist. P280 Wear protective gloves/protective clothing/eye protection/face protection. P272 Contaminated work clothing should not be allowed out of the workplace. P270 Do not eat, drink or smoke when using this product. P264 Wash with plenty of water and soap thoroughly after handling. P308 + P313 IF exposed or concerned: Get medical advice/attention.
P305 + P351 + P338 IF IN EYES: Rinse cautiously with water for several minutes. Remove contact
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	lenses, if present and easy to do so. Continue rinsing. P310 Immediately call a POISON CENTER or doctor/physician. P303 + P361 + P353 IF ON SKIN (or hair): Take off immediately all contaminated clothing. Rinse skin with water [shower]. P310 Immediately call a POISON CENTER or doctor/physician. P363 Wash contaminated clothing before reuse. P304 + P340 IF INHALED: Remove person to fresh air and keep comfortable for breathing. P301 + P330 + P331 IF SWALLOWED: Rinse mouth. Do NOT induce vomiting. P312 Call a POISON CENTER/doctor if you feel unwell. P362 + P364 Take off contaminated clothing and wash before reuse. P273 Avoid release to the environment. P405 Store locked up. P501 Dispose of contents/container into safe container in accordance with local, regional or
national regulations.

	Other Hazards:
	Unknown




	SECTION 3. COMPOSITION

	Chemical Name
	CAS No.
	% Concentration

	epoxy adduct
	Proprietary
	10 - 30 %

	isophorone diamine
	2855-13-2
	10 - 30 %

	benzyl alcohol
	100-51-6
	1 - 10 %

	4-nonylphenol, branched
	84852-15-3
	10 - 30 %

	polyoxypropylene diamine
	9046-10-0
	20 - 40 %



	SECTION 4. FIRST-AID MEASURES

	First-aid Measures Inhalation:
F INHALED: Remove person to fresh air and keep comfortable for breathing.
Skin Contact:
Flush with soap and water for a minimum of 15 minutes. Consult a physician if irritation persists or you feel unwell.
Eye Contact:
Rinse immediately with plenty of water for at least 15 minutes. Consult a physician.
Ingestion:
Rinse mouth and then drink plenty of water. Do not induce vomiting. Never induce vomiting
or give anything by mouth if the victim is unconscious or having convulsions. Immediate medical attention required.

	Most Important Symptoms and Effects, Acute and Delayed If inhaled:
May cause allergy or asthma symptoms or breathing difficulties if inhaled.
If on skin:
Harmful if in contact with the skin. Causes skin irritation. Exposure may produce an allergic reaction
If in eyes:
Causes serious eye damage.
If Ingested:
Ingestion is likely to be harmful or have adverse effects

	Immediate Medical Attention and Special Treatment:
Special Instructions:
If a physician or medical attention is required, have product container or label at hand.






 SECTION 5. FIRE-FIGHTING MEASURES	
	Extinguishing Media Suitable Extinguishing Media
In case of fire: water fog, foam, dry chemical powder, carbon dioxide (CO2)
Unsuitable Extinguishing Media
water jet

	Specific Hazards Arising from the Product
During fire, nitrous gases, fumes/smoke, isocyanates and vapors may be formed.

	Special Protective Equipment and Precautions for Fire-fighters
Self-contained breathing apparatus and turn-out gear must be worn in case of fire.




	SECTION 6. ACCIDENTAL RELEASE MEASURES

	Personal Precautions, Protective Equipment, and Emergency Procedures Clear area. Ensure adequate ventilation. Wear suitable personal protective clothing and equipment.

	Methods and Materials for Containment and Clean up
For containment, ensure adequate ventilation and absorb any spill with inert liquid binding material and dispose of waste safely.



	SECTION 7. HANDLING AND STORAGE

	Precautions for Safe Handling
Provide suitable exhaust ventilation at the processing machines. Ensure thorough ventilation of stores and work areas. Avoid aerosol formation. When handling heated product, vapors of the product should be ventilated and respiratory protection used. Wear respiratory protection when spraying. Danger of bursting when sealed gastight. Protect against moisture. If bulging of drum occurs, transfer to well-ventilated area, puncture to relieve pressure, open vent and let stand for 48 hours before resealing.

	Conditions for Safe Storage
Store in cool dry and well-ventilated place. Keep stored in accordance with local, regional, national, and international regulations. Store away from incapable materials.




	SECTION 8. EXPOSURE CONTROLS / PERSONAL PROTECTION

	Control Parameters
All protective clothing should be appropriately clean and available to dress into before work. The engineering measures or controls and PPE recommendations are only guidelines and may not apply to every situation.
Data not available. For additional information, please consult the corresponding requirements under http://www.ccohs.ca/topics/hazards/chemical/chemicals/
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	Appropriate Engineering Controls
Local exhaust ventilation required. Make up air should be supplied to balance air that is removed by local or general exhaust ventilation. Provide sufficient ventilation to keep vapors below permissible exposure limit. Emergency eye wash fountains and safety showers should be available in the immediate vicinity of any potential exposure. Ensure all national / local regulations are observed.
Individual Protection Measures
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General Measures
Do not eat, drink or smoke during work. Avoid all contact with skin or eye. If clothing comes into contact with material, do not allow out of the workplace. Clean hands and any exposed skin thoroughly after work and before breaks.
Eye / Face Protection
Use tightly sealed goggles or safety glasses with side shields which are resistant to Chemicals.
Skin Protection
Wear chemical resistant protection gloves. Wear impervious clothing as necessary to protect against coming in contact with product.
Respiratory Protection
If insufficient ventilation, wear respiratory protection.



	SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES

	Appearance
	Clear Liquid

	Odor
	Not available

	Odor threshold
	Not available

	pH
	Not available

	Melting Point
	Not available

	Initial Boiling Point / Range
	Not available

	Flash point
	>93

	Evaporation rate
	Not available

	Flammability (solid; gas)
	Not available

	Lower flammable/explosive limit
	Not available

	Upper flammable/explosive limit
	Not available

	Vapor pressure
	Not available

	Vapor density
	Not available

	Specific gravity
	0.986

	Solubility
	Partial

	Partition coefficient – n- Octanol/water
	Not available

	Auto-ignition temperature
	Not available

	Decomposition temperature
	Not available

	Viscosity
	Not available






	SECTION 10. STABILITY AND REACTIVITY

	Reactivity
	Non-reactive

	Chemical stability
	Stable under recommended handling and storage conditions

	Possibility of Hazardous reactions
	This product will polymerize if mixed with an epoxy resin. Considerable
heat can evolve.

	Conditions to avoid
	Avoid temperatures exceedingly the
flash point. Epoxy resins under uncontrolled conditions.

	Incompatible materials
	Strong oxidizing agents and acids.

	Hazardous decomposition products
	Unknown



SECTION 11. TOXICOLOGY INFORMATION
Likely Routes of Administration
Inhalation, skin contact, eye contact, ingestion.
Acute Toxicity
Oral: Harmful if swallowed.
Dermal: Harmful in contact with skin.
LD50 and LC50 Data
Not available
Skin Corrosion/Irritation
Causes skin irritation.
Serious Eye Damage/ Irritation
Causes serious eye damage
STOT (Specific Target Organ Toxicity) – Single Exposure Inhalation May cause allergy or asthma symptoms or breathing difficulties if inhaled. Aspiration Hazard
Not classified based on available data.
STOT (Specific Target Organ Toxicity) – Repeated Exposure Skin, eyes, central nervous system, respiratory system Respiratory and/or Skin Sensitization
No data Carcinogenicity Unknown
	Chemical Name
	IARC
	ACGIH®
	NTP
	OSHA

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Reproductive Toxicity
Not available
Germ Cell Mutagenicity
Not available Interactive Effects Not available

 SECTION 12. ECOLOGICAL INFORMATION	
	Toxic to aquatic life with lasting effects. This is not required by WHMIS and not required by OSHA HCS 2012



	SECTION 13. DISPOSAL CONSIDERATIONS

	Disposal Methods
Dispose of contents/container into safe container in accordance with local, regional or national regulations.



	SECTION 14. TRANSPORT INFORMATION

	
UN Number; Proper shipping name; Class(es); Packing group (PG) of the TDG Regulations:
UN3267; CORROSIVE LIQUID, BASIC, ORGANIC, N.O.S. Isophorone diamine, 4-nonylphenol, branched); CLASS 8; PG III

	UN Number; Proper shipping name; Class(es); Packing group (PG) of the IMDG (maritime):
UN3267; CORROSIVE LIQUID, BASIC, ORGANIC, N.O.S. (. Isophorone diamine, 4-nonylphenol, branched); CLASS 8; PG III; MARINE POLLUTANT

UN Number; Proper shipping name; Class(es); Packing group (PG) of the IATA (air):
UN3267; CORROSIVE LIQUID, BASIC, ORGANIC, N.O.S. Isophorone diamine, 4-nonylphenol, branched); CLASS 8; PG III; MARINE POLLUTANT



	SECTION 15. REGULATORY INFORMATION

	Not required under Canadian Regulations.



	SECTION 16. OTHER INFORMATION

	Date of Preparation
	August 2020

	Date of Last Revision
	January 4, 2023

	Revision Indicators
	The entire MDSD was change in August 2020 to be in accordance with the WHMIS 2015 which incorporates the Globally Harmonized System of Classification and Labeling
of Chemicals for Canadian Workplaces.

	References
	1. CHOHS Fact Sheets September 2016 ©CCOHS 2016
2. Supplier’s Material Safety Data Sheet(s)

	ACGIH
	American Conference of Governmental Industrial Hygienists

	ATE
	Acute toxicity estimate

	CAS
	Chemical Abstract Service

	DSL
	Domestic Substance List

	IARC
	International Agency for Research on Cancer

	IATA
	International Air Transport Association

	IMDG
	International Maritime Dangerous Goods Code

	LC
	Lethal concentration

	LD
	Lethal Dosage

	NIOSH
	National Institute for Occupational Safety and Health

	NTP
	National Toxicology Program (U.S.A.)

	OSHA
	Occupational Safety and Health Administration (U.S.A.)

	PEL
	Permissible Exposure Limit

	STEL
	Short-term Exposure Limit

	TDG
	Transport of dangerous goods in Canada

	TLV
	Threshold Limit Value

	TSCA
	Toxic Substances Control Act

	TWA
WHMIS
	Time Weighted Average
Workplace Hazardous Materials Information System






Notice: The facts stated and the recommendations made with respect to the use of this product are based on liable information. No guarantee of accuracy is made. Before using, determine the suitability of the product`s intended use. The purchaser assumes all risks and liability for losses, damage, or expenses, directly or indirectly, arising from the handling or use of the product or from any other cause. All recommendations are made on condition that SCI Coatings Inc will not be liable for any damages resulting from its use since SCI Coatings Inc cannot control the conditions under which the product will be transported, stored, handled or used by the purchaser.
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