                                             SCI-100 COVE C

	SECTION 1. IDENTIFICATION

	Product identifier
	SCI-100 COVE C

	Other Means of Identification
	N. A

	Recommended Use
	Epoxy coating aggregate

	Restrictions on Use
	Unknown

	Supplier Identifier
	SCI COATINGS INC.
2821 Boulevard Le Corbusier Laval, Québec
Canada H7L 4J5
Web: www.scicoatings.com

	Emergency Phone No.
	24-Hour Emergency Telephone Number Canada (CANUTEC): (613) 996-6666



	SECTION 2. HAZARD IDENTIFICATION

	GHS Classification

Carc. 1A
STOT RE 1
	






	Label Elements

 



[image: ]

Signal Word (GHS):                     Danger 

Hazard Statements (GHS):        May cause cancer. Causes damage to lungs through prolonged or repeated exposure.
H303: May be harmful if swallowed 

Precautionary statements
Prevention:
Obtain special instructions before use. Do not handle until safety precautions have been read and understood. Do not breathe dust, fume gas mist, vapors and spray. Wash hands, forearms and face thoroughly after handling. Do not eat, drink or smoke when using this product. Wear protective gloves, protective clothing, eye and face protection. If exposed or concern: 
Get medical advice and attention.
Dispose in a safe manner in accordance with local and national regulations.


  
	clothing and wash before reuse. P273 Avoid release to the environment. P391 Collect spillage. P501 Dispose of contents/container into safe container in accordance with local, regional or national regulations.

	Other Hazards:
	Unknown



	Chemical Name
	CAS No.
	% Concentration

	Quartz
	14808-80-7
	95-100



	SECTION 4. FIRST-AID MEASURES

	First-aid Measures 
Ingestion: May be harmful if swallowed. Do not induce vomiting advice/attention without medical advice. Never give anything by mouth to an unconscious person. Get medical. Consult a physician if symptoms develop. It may cause gastrointestinal irritation, nausea, vomiting and diarrhea.
Skin Contact: May cause mechanical irritation.
Eye Contact: May cause eye irritation. If in eyes, rinse cautiously with water for several minutes. Remove contact lenses if present and easy to do. Continue rinsing. If eye irritation persists, get medical advice/attention. 
Inhalation: May cause respiratory irritation. 


	Most Important Symptoms and Effects, Acute and Delayed If inhaled: 
May cause breathing difficulties if inhaled. Remove victim to fresh air and keep at rest in a position comfortable for breathing. Get medical advice and attention if feeling unwell.  
If on skin:
Harmful if in contact with the skin. Causes skin irritation. Exposure may produce an allergic reaction
If in eyes:
Causes serious eye damage.
If Ingested:
Ingestion is likely to be harmful or have adverse effects

	Immediate Medical Attention and Special Treatment:
Special Instructions:
If a physician or medical attention is required, have product container or label at hand.



	SECTION 5 . FIRE-FIGHTING MEASURES

	Extinguishing Media Suitable Extinguishing Media
In case of fire: Use extinguishing media appropriate for surrounding fire.
Unsuitable Extinguishing Media
Do not use a solid water stream as it may scatter and spread fire.

	Specific Hazards Arising from the Product
Fire Hazard: Product of combustion may include, and are not limited to: oxides of Carbone. 
Reactivity: Sand in mix dissolves in hydrofluoric acid, producing corrosive silicone tetrafluoride gas.
Silicates react with powerful oxidizers such as fluorine, boron trifluoride, chlorine trifluoride, manganese trifluoride and oxygen difluoride.

	Special Protective Equipment and Precautions for Fire-fighters
Wear positive-pressure self-contained breathing apparatus (SCBA) and protective fire- fighting clothing. Avoid contact with this material during fire-fighting operations. If contact
is likely, change to full chemical resistant fire-fighting clothing with self-contained breathing apparatus.
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	SECTION 6. ACCIDENTAL RELEASE MEASURES

	Personal Precautions, Protective Equipment, and Emergency Procedures Clear area. Ensure adequate ventilation. Wear suitable personal protective clothing and equipment. Vacuum or sweep up and place in a standard disposal container. 
Avoid the use of air jets, if possible, to prevent particles from becoming airborne.

	Methods and Materials for Containment and Clean up
For containment, ensure adequate ventilation and absorb any spill with inert liquid binding material and dispose of waste safely.



	SECTION 7. HANDLING AND STORAGE

	Precautions for Safe Handling
Avoid prolonged or repeated contact with skin. Avoid contact with eyes, skin, and clothing. Wash thoroughly after handling. When using, do not eat and drink. Do not use near sources of ignition. Use only non-sparking tools in work areas where the product is in use. Maintain good housekeeping methods to control dust accumulations and avoid raising dust. Provide adequate ventilation. Wear appropriate personal protective equipment. Avoid use of electric band heaters. Avoid release to the environment. Observe good industrial hygiene practices.

	Conditions for Safe Storage
Store in cool dry and well-ventilated place. Keep stored in accordance with local, regional, national, and international regulations. Store away from incapable materials.




	SECTION 8. EXPOSURE CONTROLS / PERSONAL PROTECTION

	Quartz (14808-60-7)
ACGIH                     TWA (mg/m3)             0.25 mg/m3 (respirable particule mater)
OSHA                       PEL (TWA) (mg/m3) 50 microgramme/m3
IDLH                        US IDLH (mg/m3)      50 mg/m3 respirable dust
NIOSH                     REL (TWA) (mg/m3) 0.05 mg/m3 respirable dust

Control Parameters
All protective clothing should be appropriately clean and available to dress into before work. The engineering measures or controls and PPE recommendations are only guidelines and may not apply to every situation.
Data not available. For additional information, please consult the corresponding requirements under http://www.ccohs.ca/topics/hazards/chemical/chemicals/ Appropriate Engineering Controls
Local exhaust ventilation required. Make up air should be supplied to balance air that is removed by local or general exhaust ventilation. Provide sufficient ventilation to keep vapors below permissible exposure limit. Emergency eye wash fountains and safety showers should be available in the immediate vicinity of any potential exposure. Ensure all national / local regulations are observed.
Individual Protection Measures
[image: ] [image: ] 
General Measures
Do not eat, drink or smoke during work. Avoid all contact with skin or eye. If clothing comes into contact with material, do not allow out of the workplace. Clean hands and any exposed skin thoroughly after work and before breaks.
Eye / Face Protection
Use tightly sealed goggles or safety glasses with side shields which are resistant to Chemicals.
Skin Protection
Wear chemical resistant protection gloves. Wear impervious clothing as necessary to protect against coming in contact with product.
Respiratory Protection
If insufficient ventilation, wear respiratory protection.



 
	SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES

	Appearance
	Granular solid

	Color
	White, tan, light brown

	Odor threshold
	None

	Ph
	None

	Melting Point
	1600 ˚C/2912 ˚F

	Initial Boiling Point / Range
	Not Available

	Flash point
	N. A

	Boiling point 
	2230 ˚C

	Flammability (solid; gas)
	Not available

	 Lower flammable/explosive limit
	Not available

	Upper flammable/explosive limit
	Not available

	Vapor pressure
	Not available

	 Vapor density
	Not available

	 Specific gravity @ 20 ˚C
	2.7

	Solubility
	Partial

	Partition coefficient – n- Octanol/water
	Not available

	Auto-ignition temperature
	Not available

	Decomposition temperature
	Not available



	SECTION 10. STABILITY AND REACTIVITY

	Reactivity
	Reactivity: Sand in mix dissolves in hydrofluoric acid, producing corrosive silicone tetrafluoride gas.
Silicates react with powerful oxidizers such as fluorine, boron trifluoride, chlorine trifluoride, manganese trifluoride and oxygen difluoride.

	Chemical stability
	Stable under normal conditions

	 Other 











	
	Indication of the possibility of hazardous reactions, including a statement whether the chemical will react or polymerize, which could release excess pressure or heat, or create other hazardous conditions. Also, a description of the conditions which hazardous reactions may occur. If particles become airborne during processing, handling or by other means, product may form combustible dust concentrations in air.
List of all conditions that should be avoided: Heat. Incompatible materials.
List of all classes of incompatible materials: classes of chemicals or specific substances with which the chemical could react to produce hazardous situation (strong oxidizers).
List of any known or anticipated hazardous decomposition products that could be produced because of use, storage, or heating: Carbone dioxide, organic acids.


	Incompatible materials
	Strong oxidizers. Fluorine, Chlorine trifluoride, Oxygen difluoride, Hydrofluoric acid.

	Hazardous decomposition products
	May include, and are not limited to: oxides of Carbone Silica dissolved in hydrofluoric acid producing a corrosive gas- silicon tetrafluoride. 



	SECTION 11. TOXICOLOGY INFORMATION

	Likely Routes of Administration
Inhalation, skin contact, eye contact, ingestion.
Acute Toxicity
Oral: Harmful if swallowed.
Dermal: Harmful in contact with skin.


    Acute toxicity 
[bookmark: _Hlk127901342](Oral): Not classified
Dermal: Symptoms of skin irritation may include itching or redness of the skin.
Eye contact: Not classified 
Inhalation: Not classified 
Quartz (14808-60-7)
LD50 (rat):                                          500 mg
Skin corrosion
Serious eye damage/irritation             Not classified
Respiratory or sensitization                Not classified
Germ and cell mutagenicity                Not classified 
Carcinogenicity                                   May cause cancer
Indication of whether the chemical is listed in the National toxicology Program (NTP) Report on Carcinogens (latest edition) or has been found to be a potential carcinogen in the International Agency for Research on cancer (IARC) Monographs (latest editions) or found to be a potential carcinogen by OSHA: Not listed 
IARC: Not listed
OSHA: Not regulated
STOT (Specific Target Organ Toxicity) – Single Exposure Inhalation
Not classified
Interactive Effects Not available


	SECTION 12. ECOLOGICAL INFORMATION

	This product is not harmful to aquatic organisms nor to cause long-term adverse effects in the environment. environment. This material is generally considered to be essentially non-biodegradable.



	SECTION 13. DISPOSAL CONSIDERATIONS

	Disposal Methods
Dispose of contents/container into safe container in accordance with local, regional or national regulations.



	SECTION 14. TRANSPORT INFORMATION

	
Department of Transportation (DOT) and Transportation of Dangerous Goods (TDG) in accordance with DOT/TDG: Not regulated







	SECTION 15. REGULATORY INFORMATION

	Not required under Canadian Regulations.



	SECTION 16. OTHER INFORMATION

	Date of Preparation
	August 2022

	Date of Last Revision
	January 4, 2023

	Revision Indicators
	The entire MDSD was change in August 2020 to be in accordance with the WHMIS 2015 which incorporates the Globally Harmonized System of Classification and Labeling
of Chemicals for Canadian Workplaces.

	References
	1. CHOHS Fact Sheets September 2016 ©CCOHS 2016
2. Supplier’s Material Safety Data Sheet(s)

	ACGIH
	American Conference of Governmental Industrial Hygienists

	ATE
	Acute toxicity estimate

	CAS
	Chemical Abstract Service

	DSL
	Domestic Substance List

	IARC
	International Agency for Research on Cancer

	IATA
	International Air Transport Association

	IMDG
	International Maritime Dangerous Goods Code

	LC
	Lethal concentration

	LD
	Lethal Dosage

	NIOSH
	National Institute for Occupational Safety and Health

	NTP
	National Toxicology Program (U.S.A.)

	OSHA
	Occupational Safety and Health Administration (U.S.A.)

	PEL
	Permissible Exposure Limit

	STEL
	Short-term Exposure Limit

	TDG
	Transport of dangerous goods in Canada

	TLV
	Threshold Limit Value

	TSCA
	Toxic Substances Control Act

	TWA
	Time Weighted Average

	WHMIS
	Workplace Hazardous Materials Information System




Notice: The facts stated and the recommendations made with respect to the use of this product are based on liable information. No guarantee of accuracy is made. Before using, determine the suitability of the product`s intended use. The purchaser assumes all risks and liability for losses, damage, or expenses, directly or indirectly, arising from the handling or use of the product or from any other cause. All recommendations are made on condition that SCI Coatings Inc will not be liable for any damages resulting from its use since SCI Coatings Inc cannot control the conditions under which the product will be transported, stored, handled or used by the purchaser.
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