SCI-100 COVE A 

	SECTION 1. IDENTIFICATION

	Product identifier
	SCI-100 COVE A 

	Other Means of Identification
	N. A

	Recommended Use
	Epoxy coating

	Restrictions on Use
	Unknown

	Supplier Identifier
	SCI COATINGS INC.
2821 Boulevard Le Corbusier Laval, Québec
Canada H7L 4J5
Web: www.scicoatings.com

	Emergency Phone No.
	24-Hour Emergency Telephone Number Canada (CANUTEC): (613) 996-6666



	SECTION 2. HAZARD IDENTIFICATION

	Classification
	Skin Sensitization Category 1B Skin Corrosion/irritation Category 2
Serious eye damage/irritation Category 2A Acute Toxicity, Oral Category 5
Hazardous to the aquatic environment - acute Category 2 Hazardous to the aquatic environment - chronic Category 2

	Label Elements
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Signal Word
Warning

Hazard Statements
H303: May be harmful if swallowed H315: Causes skin irritation
H317: May cause an allergic skin reaction H319: Causes serious eye irritation
H401: Toxic to aquatic life
H411: Toxic to aquatic life with long lasting effects
Precautionary statements
Prevention:
P261 Avoid breathing dust/fume/gas/mist/vapors/spray. P264 Wash with plenty of water and soap thoroughly after handling. P272 Contaminated work clothing should not be allowed out of the workplace. P280 Wear protective gloves/eye protection. P305 + P351 + P338 IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do so. Continue rinsing. P337 + P313 If eye irritation persists: Get medical advice/attention. P302 + P352 IF ON SKIN: Wash with plenty of water. P333 + P313 If skin irritation or rash occurs: Get medical advice/attention. P312 IF
SWALLOWED: Call a POISON Center/doctor/…if you feel unwell. P362 + P364 Take off contaminated
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	clothing and wash before reuse. P273 Avoid release to the environment. P391 Collect spillage. P501 Dispose of contents/container into safe container in accordance with local, regional or national regulations.

	Other Hazards:
	Unknown



	Chemical Name
	CAS No.
	% concentration

	Reaction product: bisphenol-A-
(epichlorohydrin) epoxy resin
	25085-99-8
	60 - 100

	alkyl (C12-C14) glycidyl ether
	68609-97-2
	1 - 10

	Benzyl Alcohol
	100-51-6
	1 - 10



	SECTION 4. FIRST-AID MEASURES

	First-aid Measures Ingestion:
IF SWALLOWED: Call a POISON Center/doctor/…if you feel unwell.
Skin Contact:
Flush with soap and water for a minimum of 15 minutes. Consult a physician if irritation persists or you feel unwell.
Eye Contact:
Rinse immediately with plenty of water for at least 15 minutes. Consult a physician.

	Most Important Symptoms and Effects, Acute and Delayed If inhaled:
May cause allergy or asthma symptoms or breathing difficulties if inhaled.
If on skin:
Harmful if in contact with the skin. Causes skin irritation. Exposure may produce an allergic reaction
If in eyes:
Causes serious eye damage.
If Ingested:
Ingestion is likely to be harmful or have adverse effects

	Immediate Medical Attention and Special Treatment:
Special Instructions:
If a physician or medical attention is required, have product container or label at hand.



	SECTION 5. FIRE-FIGHTING MEASURES

	Extinguishing Media Suitable Extinguishing Media
In case of fire: water fog, foam, dry chemical powder, carbon dioxide (CO2)
Unsuitable Extinguishing Media
water jet

	Specific Hazards Arising from the Product
During fire, smoke may contain the original material in addition to combustion products of varying composition which may be toxic and/or irritating.

	Special Protective Equipment and Precautions for Fire-fighters
Wear positive-pressure self-contained breathing apparatus (SCBA) and protective fire- fighting clothing. Avoid contact with this material during fire-fighting operations. If contact
is likely, change to full chemical resistant fire-fighting clothing with self-contained breathing apparatus.




	SECTION 6. ACCIDENTAL RELEASE MEASURES

	Personal Precautions, Protective Equipment, and Emergency Procedures Clear area. Ensure adequate ventilation. Wear suitable personal protective clothing and equipment.

	Methods and Materials for Containment and Clean up
For containment, ensure adequate ventilation and absorb any spill with inert liquid binding material and dispose of waste safely.



	SECTION 7. HANDLING AND STORAGE

	Precautions for Safe Handling
Avoid prolonged or repeated contact with skin. Avoid contact with eyes, skin, and clothing. Wash thoroughly after handling. When using, do not eat, drink or smoke. Provide adequate ventilation. Wear appropriate personal protective equipment. Avoid use of electric band heaters. Avoid release to the environment. Observe good industrial hygiene practices.

	Conditions for Safe Storage
Store in cool dry and well-ventilated place. Keep stored in accordance with local, regional, national, and international regulations. Store away from incapable materials.




	SECTION 8. EXPOSURE CONTROLS / PERSONAL PROTECTION

	Control Parameters
All protective clothing should be appropriately clean and available to dress into before work. The engineering measures or controls and PPE recommendations are only guidelines and may not apply to every situation.
Data not available. For additional information, please consult the corresponding requirements under http://www.ccohs.ca/topics/hazards/chemical/chemicals/ Appropriate Engineering Controls
Local exhaust ventilation required. Make up air should be supplied to balance air that is removed by local or general exhaust ventilation. Provide sufficient ventilation to keep vapors below permissible exposure limit. Emergency eye wash fountains and safety showers should be available in the immediate vicinity of any potential exposure. Ensure all national / local regulations are observed.
Individual Protection Measures
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General Measures
Do not eat, drink or smoke during work. Avoid all contact with skin or eye. If clothing comes into contact with material, do not allow out of the workplace. Clean hands and any exposed skin thoroughly after work and before breaks.
Eye / Face Protection
Use tightly sealed goggles or safety glasses with side shields which are resistant to Chemicals.
Skin Protection




	Wear chemical resistant protection gloves. Wear impervious clothing as necessary to protect against coming in contact with product.
Respiratory Protection
If insufficient ventilation, wear respiratory protection.



	SECTION 9. PHYSICAL AND CHEMICAL PROPERTIES

	Appearance
	Clear Liquid

	Odor
	Not available

	Odor threshold
	Not available

	pH
	Not available

	Melting Point
	Not available

	Initial Boiling Point / Range
	Not Available

	Flash point
	>93

	Evaporation rate
	Not available

	Flammability (solid; gas)
	Not available

	Lower flammable/explosive limit
	Not available

	Upper flammable/explosive limit
	Not available

	Vapor pressure
	Not available

	Vapor density
	Not available

	Specific gravity
	1.14

	Solubility
	Partial

	Partition coefficient – n- Octanol/water
	Not available

	Auto-ignition temperature
	Not available

	Decomposition temperature
	Not available

	Viscosity
	Not available



	SECTION 10. STABILITY AND REACTIVITY

	Reactivity
	Non-reactive

	Chemical stability
	Stable under recommended handling and storage conditions

	Possibility of Hazardous reactions
	This product will polymerize if mixed with an amine. Considerable heat can
evolve.

	Conditions to avoid
	Avoid temperatures exceedingly the
flash point. Avoid unintended contact with amines.

	Incompatible materials
	Strong oxidizers, strong alkalis, strong mineral acids, amines.

	Hazardous decomposition products
	Unknown



	SECTION 11. TOXICOLOGY INFORMATION

	Likely Routes of Administration
Inhalation, skin contact, eye contact, ingestion.
Acute Toxicity
Oral: Harmful if swallowed.
Dermal: Harmful in contact with skin.




LD50 and LC50 Data
Not available
Skin Corrosion/Irritation
Causes skin irritation.
Serious Eye Damage/ Irritation
Causes serious eye damage
STOT (Specific Target Organ Toxicity) – Single Exposure Inhalation
No data
Aspiration Hazard
Not classified based on available data.
STOT (Specific Target Organ Toxicity) – Repeated Exposure
No data
Respiratory and/or Skin Sensitization
May irritate mucous membranes, eyes, nose, and respiratory passages. May cause asthma attack to persons with pre-existing bronchial hyper reactivity. Exposure to high concentrations may lead to bronchitis, bronchial spasm and pulmonary oedema.
Effects are usually reversible. May cause C.N.S. depression with symptoms of nausea, light-headedness, drowsiness, dizziness, loss of coordination Carcinogenicity
Unknown Reproductive Toxicity Not available
Germ Cell Mutagenicity
Not available Interactive Effects Not available


	SECTION 12. ECOLOGICAL INFORMATION

	Hazardous to aquatic environment This is not required by WHMIS
This is not required by OSHA HCS 2012



	SECTION 13. DISPOSAL CONSIDERATIONS

	Disposal Methods
Dispose of contents/container into safe container in accordance with local, regional or national regulations.



	SECTION 14. TRANSPORT INFORMATION

	

	
UN Number; Proper shipping name; Class(es); Packing group (PG) of the TDG Regulations:
UN3082; ENVIRONMENTALLY HAZARDOUS SUBSTANCE, LIQUID, N.O.S. (bisphenol-A-(epichlorohydrin) epoxy resin); CLASS 9; PG III

	UN Number; Proper shipping name; Class(es); Packing group (PG) of the IMDG (maritime):
UN3082; ENVIRONMENTALLY HAZARDOUS SUBSTANCE, LIQUID, N.O.S. (bisphenol-A-(epichlorohydrin) epoxy resin); CLASS 9; PG III; MARINE POLLUTANT

UN Number; Proper shipping name; Class(es); Packing group (PG) of the IATA (air):
UN3082; ENVIRONMENTALLY HAZARDOUS SUBSTANCE, LIQUID, N.O.S. (bisphenol-A-(epichlorohydrin) epoxy resin); CLASS 9; PG III; MARINE POLLUTANT




	SECTION 15. REGULATORY INFORMATION

	Not required under Canadian Regulations.



	SECTION 16. OTHER INFORMATION

	Date of Preparation
	August 2022

	Date of Last Revision
	January 4, 2023

	Revision Indicators
	The entire MDSD was change in August 2020 to be in accordance with the WHMIS 2015 which incorporates the Globally Harmonized System of Classification and Labeling
of Chemicals for Canadian Workplaces.

	References
	1. CHOHS Fact Sheets September 2016 ©CCOHS 2016
2. Supplier’s Material Safety Data Sheet(s)

	ACGIH
	American Conference of Governmental Industrial Hygienists

	ATE
	Acute toxicity estimate

	CAS
	Chemical Abstract Service

	DSL
	Domestic Substance List

	IARC
	International Agency for Research on Cancer

	IATA
	International Air Transport Association

	IMDG
	International Maritime Dangerous Goods Code

	LC
	Lethal concentration

	LD
	Lethal Dosage

	NIOSH
	National Institute for Occupational Safety and Health

	NTP
	National Toxicology Program (U.S.A.)

	OSHA
	Occupational Safety and Health Administration (U.S.A.)

	PEL
	Permissible Exposure Limit

	STEL
	Short-term Exposure Limit

	TDG
	Transport of dangerous goods in Canada

	TLV
	Threshold Limit Value

	TSCA
	Toxic Substances Control Act

	TWA
	Time Weighted Average

	WHMIS
	Workplace Hazardous Materials Information System




Notice: The facts stated and the recommendations made with respect to the use of this product are based on liable information. No guarantee of accuracy is made. Before using, determine the suitability of the product`s intended use. The purchaser assumes all risks and liability for losses, damage, or expenses, directly or indirectly, arising from the handling or use of the product or from any other cause. All recommendations are made on condition that SCI Coatings Inc will not be liable for any damages resulting from its use since SCI Coatings Inc cannot control the conditions under which the product will be transported, stored, handled or used by the purchaser.
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